|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  | | --- | --- | | Product Description | Wood-Plastic Composite | | Dimension | 7 in x 48 in | | Thickness | 6.5 mm | | Wear Thickness | 0.5 mm 20 mil | | Color | 6 Available | | Planks / Carton | 10 | | Square / Plank | 2.33 | |  |

|  |  |  |
| --- | --- | --- |
| **Fire Resistance** | *Class C – Pass* | ASTM 648 |
| **Coefficient of Friction** | *Pass* | DIN 51130 / ASTM D2047-04 |
| **Smoke Density** | *Pass* | ASTM E662-09 |
| **Short Term Indentation** | *Pass* | ASTM F1914—98 |
| **Static Load** | *Pass* | EN 433 / ASTM F970-07 |
| **Stain Resistance** | *Pass* | ASTM F925 |
| **Peel Resistance** | *Pass* | EN 431 |
| **Shear Resistance** | *Pass* | EN 532 |
| **Color Fastness to Light** | *Pass* | EN 649 |
| **Dimensional Stability** | *Pass* | EN 434 |
| **Wear Resisistance** | *High* | ASTM F510-93 |
| **Formaldehyde Emission (air)** | *None Detected – E1 Rating\** | EN 7171-1 |

*\* E1 Standard not to exceed 0.124 mg/m3 air  
\* Method Detection Limit 0.080 mg/m3 air*